

Contact: [**Clyne Media, Inc.**](http://www.clynemedia.com/audiotechnica/)

Tel: (615) 662-1616

**Audio-Technica displays AT2040USB Hypercardioid Dynamic USB Microphone**

*The NAMM Show, Anaheim, CA, January 25, 2024* — [Audio-Technica](https://www.audio-technica.com/en-us/) (booth 15314), a leading innovator in transducer technology for over 60 years, is displaying its [AT2040USB](https://www.audio-technica.com/en-us/at2040usb) Hypercardioid Dynamic USB Microphone – a recent addition to A-T’s comprehensive lineup of 20 Series content creation products. The AT2040USB microphone combines the broadcast-quality performance of the AT2040 dynamic microphone with plug-and-play USB Type-C™ functionality, making it easy for podcasters, streamers, and other content creators to achieve professional results. The microphone connects directly to the user’s computer for immediate use—no audio interface or additional cabling is required.

With its crystal-clear studio sound, the easy-to-use AT2040USB is the ideal microphone for content creators looking to gain a professional edge and increase engagement. The mic has a high-resolution A/D converter with a sampling rate of up to 24 bits/96 kHz for extremely clear and natural sound, and its highly directional, hypercardioid pickup pattern isolates the user’s voice from surrounding noise, ensuring the focus remains on the spoken content. Gamers who stream and chat with followers will appreciate the isolation from common ambient noise, such as the hum of a computer fan.

The microphone’s robust metal body includes an integrated shock mount to attenuate unwanted noise and vibration, while its internal pop filter (a multistage foam mesh windscreen) protects against harsh spoken sounds. Additionally, its low-cut filter eliminates low-frequency sound for additional reduction of vibration and surrounding environmental noise. The AT2040USB is also equipped with a headphone jack to enable real-time monitoring of the audio (with zero latency), as well as a soft-touch mute button for quick, reliable muting at the microphone. A mix control dial adjusts the balance between the microphone audio and a computer sound source. A two-state LED indicator ring lights blue when the mic is powered on and ready to capture audio and lights red when it is muted.

The AT2040USB comes with a USB cable (USB Type-C to USB Type-A) and USB adapter (USB Type-A to USB Type-C) for plug-and-play functionality. The AT8458a shock mount (sold separately) can also be used with the microphone to further reduce any noise, shock, or vibration that might be transmitted through a mic stand, boom, or mount.

For more information, please visit [www.audio-technica.com](https://www.audio-technica.com/en-us/).

*…ends 358 words*

Photo file 1: AT2040USB\_PR\_01.JPG

Photo caption 1: AT2040USB Hypercardioid Dynamic USB Microphone

Photo file 2: AT2040USB\_PR\_02.JPG

Photo caption 2: AT2040USB Hypercardioid Dynamic USB Microphone (application photo)

Photo file 3: AT2040USB\_PR\_03.JPG

Photo caption 3: AT2040USB Hypercardioid Dynamic USB Microphone, shown with other A-T 20 Series content creation products

Audio-Technica was founded in 1962 with the mission of producing high-quality audio for everyone. A leading innovator in transducer technology, Audio-Technica is renowned for the design and manufacture of microphones, wireless microphones, headphones, mixers, and turntables for the audio industry. We work to expand the limits of audio technology, pursuing an ever-changing purity of sound that creates connections and enriches lives. Visit [https://www.audio-technica.com/](https://www.audio-technica.com/en-us/).

*—For more information on the complete range of Audio-Technica products, contact Jamie Bobek, Audio-Technica U.S., Inc., 1221 Commerce Drive, Stow, OH 44224. Tel: (330) 686-2600; Fax: (330) 688-3752; Web:* [*www.audio-technica.**com*](https://www.audio-technica.com/en-us/)

*— For further information regarding product availability and pricing in Europe, contact Tanya Williams (*[*TWilliams@audio-technica.eu*](mailto:TWilliams@audio-technica.eu)*).*